**ADDENDUM TO BID PACKAGE**

It is the intent of the City of Muskegon (“Agency”) to purchase roofing materials for the City of Muskegon 2021 Water Filtration Plant Upgrades (“Project”) located at 1900 Beach St. Muskegon, MI directly from Garland Inc., based upon the Agency’s participation in the U.S. Communities / OMNIA Government Purchasing Alliance’s program for Roofing Supplies and Related Products and Services, as priced by and awarded to Garland/DBS, Inc., resulting from the competitively solicited Sealed Bid # PW1925 issued by the Racine County Board of Commissioners.

For this project, the Garland Representative will provide the City of Muskegon with the amounts and pricing for the Garland Material that will be needed for the project:

**Water Filtration Plant – Section #3 & #11 & Harvey St. Pump**

**Base Bid – 2-ply Modified Bitumen w/ Coal Tar Flood and Gravel**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Product #** | **Product Name** | **Unit / Size** | **Coverage Rate** | **Quantity** |
| 4364 | Versiply 80 | Roll | 100 SF |  |
| 7343-5 | Black-Knight  | 5-gal | 100 SF |  |
| 7425-5 | Silver-Flash Mastic | 5-gal | 7 lnr. ft. / gal |  |
| 4840-6 | GarMesh | Roll | 75 SF |  |
| 7411-5 | Garla-Brite | 5-gal | 500 SF |  |
| 7336-5 | Weatherking Adhesive | 5-gal | 2.5 gal./ sq. |  |
| 7110-5 | Flashing Bond | 5-gal | 4-6 gal./ sq. |  |
| 4381 | StressPly IV | Roll | 75 SF |  |
| 2138-BLK | Greenlock Structural Adhesive | Tube | 10 oz. tube |  |

**Alternate Bid – 2-ply Modified Bitumen Smooth w/ Aluminized Coating**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Product #** | **Product Name** | **Unit / Size** | **Coverage Rate** | **Quantity** |
| 4364 | Versiply 80 | Roll | 100 SF |  |
| 7425-5 | Silver-Flash Mastic | 5-gal | 7 lnr. ft. / gal |  |
| 4840-6 | GarMesh | Roll | 75 SF |  |
| 7411-5 | Garla-Brite | 5-gal | 500 SF |  |
| 7336-5 | Weatherking Adhesive | 5-gal | 2.5 gal./ sq. |  |
| 7110-5 | Flashing Bond | 5-gal | 4-6 gal./ sq. |  |
| 4382 | StressPly IV Mineral | Roll | 75 SF |  |
| 2138-BLK | Greenlock Structural Adhesive | Tube | 10 oz. tube |  |

**Water Filtration Plant – Harvey St. Underground**

**Base Bid – 2-ply Modified Bitumen**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Product #** | **Product Name** | **Unit / Size** | **Coverage Rate** | **Quantity** |
| 4411-80 | StressBase 80 | Roll | 150 SF |  |
| 4360 | StressPly  | Roll  | 100 SF |  |

**PLEASE NOTE:**

1. It is the responsibility of the bidder to obtain any product-related information from the Garland representative prior to bid submission.
2. Additional Garland Material needed for this project needs to be included in the contractor’s base bid.
3. Contractor will EXCLUDE the above pricing from their base bid due to the fact the City will be buying the material directly from Garland through the US Communities Contract